AFU (AMI Firmware Update for FreeBSD) is a utility used 
to update the system BIOS under various operating systems.  

Note: AFU only works for AMIBIOS with SMI FLASH support.

Current version: 1.33

The package includes:

- AFUBSD


How to run the utility under FreeBSD (version 3.0 and above)
-------------------------------------------
1. Run the file AFUBSD (to execute the command from the current directory type ./AFUBSD)


 Usage 
------------------------------------------------------------------
afubsd /i<ROM filename> [/o<save ROM filename>] [/n] [/p[b][n][c]] [/s] [/k[N]] [/c[N]] [/q] [/h] [/t] [/u<ROM filename>] [/d]

        /n    - Don't check ROM ID
        /pbnc -
                b - Program Boot Block
                n - Program NVRAM
                c - Destroy System CMOS
        /k    - Program all non-critical blocks only
        /kN   - Program N'th non-critical block only (from k0 upto k7)
        /s    - Leave signature in BIOS
        /q    - Silent execution
        /h    - Print help
        /t    - Display ROM ID string
        /c    - Program Main BIOS and all Non-critical blocks
        /cN   - Program Main BIOS and N'th Non-critical block (from c0 upto c7)
        /d    - Compare ROM file (skips flashing)
        /u<ROM filename>   -Display ROM ID 

