//*****************************************************************************
//
//                   INTEL CORPORATION PROPRIETARY INFORMATION
//       This software is supplied under the terms of a license agreement or
//       nondisclosure agreement with Intel Corporation and may not be copied
//       or disclosed except in accordance with the terms of that agreement.
//         Copyright (c) 2006 Intel Corporation. All Rights Reserved.
//*****************************************************************************

//
// File Header Information
//

_LF_NAME       'Main Board'  // The name for this load file
_LF_VERSION    '0.03'       // Version of this load file
_LF_FMT_VER    '1.50'       // Version of the load file format
_IPMI_VERSION  '2.00'       // IPMI format version

//
// FRU Area Header 
//

_FRU (                      // FRU data for the Main Board
_FRU_TITLE     'Basbrd Mgt Ctlr' // FRU title
_START_ADDR    0000         // Start Address
_DATA_LEN      00D0         // Data Length
_NVS_TYPE      'IMBDEVICE'  // AT24C64 SEEPROM
_DEV_ID        00           // Device ID
_DEV_BUS       FF           // I2C address 
_DEV_ADDRESS   20           // Controller Address

_SEE_COMMON
   01                 // Common Header Format Version
   01                 // Internal Use Area Starting Offset (in multiples of 8 bytes)
   02                 // Chassis Info Area Starting Offset (in multiples of 8 bytes)
   07                 // Board Info Area Starting Offset (in multiples of 8 bytes)
   10                 // Product Info Area Starting Offset (in multiples of 8 bytes)
   00                 // MultiRecord Area Starting Offset (in multiples of 8 bytes)
   00                 // Pad
   E5                 // Common Header Checksum

_SEE_INTERNAL
   01 00 00 00 00 00 00 01 // 0h - 7h

_SEE_CHASSIS
   01                 // Chassis Info Area Format Version Bit Fields
   05                 // Chassis Info Area Length (in multiples of 8 bytes)
   17                 // Chassis Type
   C0                 // Chassis Part Number
   C0                 // Chassis Serial Number
   C0                 // Chassis Custom Field
   C1                 // End of field marker

_SEE_BOARD
   01                 // Board Info Area Format Version Bit Fields
   09                 // Board Info Area Length (in multiples of 8 bytes)
   00                 // Language Code
   00 00 00           // Mfg. Date/Time	
   C5                 // Board Manufacturer	type/length byte
   'Intel'            // 5 digit ASCII Board Manufacturer name
   CA                 // Board Product Name	type/length byte
   'S5000XAL0 '				// Board Product Name
   CC                 // Board Serial Number
   '............'     // Mock-up 12 digit ASCII board serial number
   CA                 // Board Part Number
   '..........'       // Mock-up 10 digit ASCII board part number
   CC                 // FRU File ID --type/length byte--
   'FRU Ver 0.03'     // FRU Version Number
   C0                 // Board Custom Field --type/length byte--
   C1                 // End of field marker

_SEE_PRODUCT
   01                 // Product Info Area Format Version Bit Fields
   0A                 // Product Info Area Length (in multiples of 8 bytes)
   00                 // Language Code
   C5                 // Product Manufacturer Name
   'Intel'            // 5 digit ASCII Board Manufacturer name
   C8                 // Product name --type/length byte--
   'S5000XAL'
   CA                 // Product Part/Model Number --type/length byte--
   '..........'				// 10-bytes
   C0                 // Product Version
   C9                 // Product Serial Number --type/length byte--
   '.........'				// 9-bytes
   C0                 // Asset Tag --type/length byte--
   C0                 // FRU File ID
   C0                 // Product Custom Field
   C1                 // End of field marker

)

//** End of FRU for Main board AT24C64*****************************************
