ServerConductor/Blade Server Manager Description and Reference

### 3.1.4 Port numbers used by ServerConductor

When ServerConductor programs are installed, the default port numbers listed below are used.

You can use the services file to change a port to be used. You must set a port that is not used by any other application.

Port number | Service name | Description
--- | --- | ---
1099/tcp | -- | Communication to the Java Gateway Web Console Servelet Java Gateway
20075/tcp | sys_agt_port | Communication to the agent service - Manager service agent service - Hardware maintenance registration application (MRegAgt.exe) agent service
20076/tcp | sys_ra_port | Communication to the manager service - Agent service manager service - Managed client manager service
20077/tcp | sys_gui_port | Communication to the console - Manager service console service
20078/tcp | sys_web_port | Communication to the Web gateway service Manager service Web gateway service
20079/tcp | sys_svalt_port | Communication to the manager service SVP manager service
20299/tcp | sys_altact_port | Communication to the alert action service - Manager service alert action service
623/udp | -- | Communication to BMC - Manager service BMC
22311/tcp | sys_agtssmp_port | For hardware maintenance

All Rights Reserved. Copyright (C) 2006, Hitachi, Ltd.