ServerConductor/Blade Server Manager Description and Reference

### 15.8.3 Setting the manager service

The manager service settings are managed in the Manager service settings window.

To display the Manager service settings window:

1. In the Host management window, from the Settings menu, choose Manager service settings.
   The Manager service settings window appears.

   Figure 15-30 Manager service settings window

Clicking the Network setting menu displays the following window:

Figure 15-31 Network setting

You can set the following information in this window:

Item | Setting
--- | ---
Command timeout value | Set the time (in seconds) to wait for a reply to the command transmission from the manager service to the agent service. The permitted value range is from 1 to 600. The default is 90 seconds.

All Rights Reserved. Copyright (C) 2006, Hitachi, Ltd.