ServerConductor/Blade Server Manager Description and Reference

### 3.4.1 Setting passwords (manager service)

You can set passwords for logging on to the manager service from the management console.

Item | Setting
--- | ---
Administrator | Click the Administrator button to set the administrator password.
Sub Administrator | Click the Sub Administrator button to set the sub-administrator password.

Clicking the Administrator or Sub Administrator button displays the Set Password dialog box (if a password has already been set, the Change Password dialog box appears).

An administrator can monitor host status and change settings. A sub-administrator can monitor host status but cannot change settings. Set a password using 1-16 alphanumeric characters, spaces, and symbols. Note that passwords must be set.

All Rights Reserved. Copyright (C) 2006, Hitachi, Ltd.