Notes:
1.	Support West Union and Rosamond platforms only.
2.	Support new linkstep feature on West Union platform.
3.	IPM ICH control will not work under XP64.

IPM Installation Steps:
1.	Step1.
	Install Intel Power Manager by clicking its SetupLauncher.exe, which will install IPM solution based on 32bit / 64bit OS and WU/RM platform.
2.	Step2.
	Restart PC. IPM will provide an icon in Windows system tray, and a quick switch menu by pressing hotkey Alt+F3.


Appendix A: Feature list of IPM software only version:
1.	Scheme based power management. Support power scheme operations ¨C New, Edit, Delete, icon selection.
2.	Support dynamic configuration. Most of features can be customized without rebuild.
3.	Support basic power scheme settings of Windows(XP and Vista), including:
	3.1	Turn off Display after a time
	3.2	Stop hard disk rotation after a time
	3.3	Enter System standby after a time
	3.4	Enter System hibernation after a time(must enable Hibernation in OS power option)
4.	Support to adjust CPU frequency by using Intel SpeedStep technology
5.	Support Intel DPST technology. (Intel Graphics adapter and driver must be installed before IPM runs.)
6.	Support Intel Link Step technology. (Need Intel 82566 Ethernet adapter and driver)
7.	Support to control backlight level of LCD. (Need BIOS, driver and OS support)
8.	Support to turn on/off USB devices. (Need Intel ICH8 or above)
9.	Support to adjust NIC speed.
10.	Support to display basic and advanced battery information. (Need BIOS support)
