This release note and the software that accompanies it are copyright (c) 2010, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported Hardware
==========================
(1) Intel(R) Compute Module MFS5000SI

(2) Intel(R) Compute Module MFS5520VI

===================
Package Information
===================
Driver Version = 1.31.02.00
OS supported = Windows* 2003 (x86, x64), Windows* 2008 (x86, x64, R2x64)

=========
Attention
=========
N/A

==================
Known Restrictions
==================
N/A

=======================
Contents on the package
=======================
The following files(or folders) are included in this package:

Name			Description
readme.txt		This file
License_v2.pdf		Software license
/Server 2003 32-bit	x86 version drivers for Windows* 2003 32-bit
/Server 2003 64-bit	x64 version drivers for Windows* 2003 64-bit
/Server 2008 32-bit	x86 version drivers for Windows* 2008 32-bit
/Server 2008 64-bit	x64 version drivers for Windows* 2008 64-bit
/Server 2008 R2 64-bit	x64 version drivers for Windows* 2008 R2 64-bit

=========================
Installation Instructions
=========================

The following procedure describes how to provide the driver during installation of Windows 2003 system:

NOTE: You will need a USB floppy drive in order to provide the driver during Windows installation. Some models of floppy drives have known limitations that result in driver installation failures. Intel recommends using USB floppy drives listed on the Tested Hardware and Operating Systems list for the serverboard you are using.

1. Extract package contents to a floppy diskette.
2. Start the Windows 2003 installation by booting from the Windows installation CD-ROM.
3. Press <F6> when the screen displays: "Press F6 if you need..." 
Note: You must press <F6> for the system to recognize the new driver.
4. Choose <S> to specify an additional device when the screen displays:
"Setup could not determine the type of one or more mass storage devices..."
Note: If this screen is not displayed as the first user input, then pressing <F6> was not seen by the setup program. Reboot the system, and return to step 2.
5. The system prompts for the manufacturer-supplied hardware support disk. Insert the floppy diskette containing the Windows 2003 device driver, and press <Enter>.
6. Scroll down the list until the appropriate selection for your system, then click <OK>.
7. Continue with the normal installation procedure.
If installation fails after the first reboot, try another model of USB floppy drive from the tested list.

================

Installation of the driver after the operating system is installed, for Windows Server 2008 system:

1. Boot into applicable Windows OS. Copy the appropriate driver files to a folder on the system.
2. Right-click "My Computer" on the Start menu and select "Manage".
3. On the left pane, under "Diagnostics" select "Device Manager".
4. On the right pane, under "Storage Controllers" select "LSI Adapter, SAS 3000 Series, 4-port with 1064E".
5. Right-click "LSI Adapter, SAS 3000 Series, 4-port with 1064E" and select "Update Driver Software".
6. Select "Browse my computer for driver software".
7. Select "Browse", find the folder containing the driver files, select "OK" and select "Next".
8. Select "Close".  You will be prompted to reboot, select "Yes".
9. After reboot driver installation is complete.ystem.

============
Known Issues
============
None

*Third-party trademarks are the property of their respective owners.