Intel® Astor Chassis and Intel® Cabrillo-C Chassis
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your products
  End of Interactive Support Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail

Technical specifications
  Astor Technical Product Specification [PDF]
  Astor Technical Product Specification update [PDF]
  Cabrillo-C Technical Product Specification [PDF]
  Cabrillo-C Technical Product Specification update [PDF]

Installation and use
  Astor chassis features
    - Two external 5.25" drive bays (not certified for hard drive use)
    - External hot swap 3.5" drive bay supporting five 10K RPM 1" high SCA hard drives
    - Physical security (lockable back and hot swap drive bay) with chassis-intrusion monitoring through LANDesk* Server Manager
    - Three instrumented (tachometer) 92 mm system cooling fans monitored through LANDesk* Server Manager
    - Compliance with most major safety and EMC regulations worldwide when properly integrated with the Intel® N440BX Server Board
    - Design based on the Intel® Columbus II Chassis with improved ease of integration/serviceability
    - Detailed system integration manual
  Cabrillo-C chassis features
    - Designed for the Intel® C440GX server board
    - Three external 5.25" drive bays (not certified for hard drive use)
    - External hot swap 3.5" drive bay with support for six Ultra2 SCSI 10K RPM 1" high SCA2 hard drives.
    - Physical security (lockable back and hot swap drive bay) with chassis-intrusion monitoring through Intel® Server Control (ISC)+
    - Advanced cooling system with four fans, optimized peripheral bay placement and coordinated air intake and exhaust channels.
    - Compliance with most major safety and EMC regulations worldwide when properly integrated with the C440GX+
    - Detailed system integration manual
  Astor Product Guide [PDF]
  Cabrillo-C Product Guide [PDF]