This release note and the software that accompanies it are copyright (c) 2011, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.
This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation. 

==========================
Supported RAID Controllers
==========================
This download supports SGXPCIESAS-R-EXT-Z, SGXPCIESAS-R-INT-Z and X4620A Sun Blade RAID 5 Expansion Module, please verify that this package has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
Version = 6.10.0 - 18707
Supported OS = Windows_x64

==================
Known Restrictions
==================
N/A

=======================
Contents on the package
=======================
manager
	setup_sstrm_x86.exe

================================
Usage/Installation Instructions:
================================
N/A

============
Known Issues
============
Version 6.10.0 - 17557
	ADPml12017 - Discrepancy in the size reported during array creation time in the SSM GUI and CLI after the array was created. The array was always created with 10MB less than what was originally shown in the SSM GUI.

Version 6.10.0 - 17536
	BLINK Logical Device feature in Sun RAID Manager does not blink correct members of logical array.? This problem is observed on the StorageTek J4500 Enclosure.? LOKI enclosure does not appear to have this problem.? Blinking of physical device appears correct.

Version 6.10.0 - 17533
	BLINK Logical Device feature in Sun RAID Manager does not blink correct members of logical array.? This problem is observed on the StorageTek J4600 Enclosure.? LOKI enclosure does not appear to have this problem.? Blinking of physical device appears correct.

Version 6.10.0 - 17523
	6669319 (9572) -  Sun RAID Manager shows 4 enclosures for a 2 Loki tray cascade.

Version 6.10.0 - 17509
	6640462 (ADPml09041) - Sun RAID Manager reports LOKI Device Status with fewer details than we provide for Alamo Device Status.

=============
Fixes/Updates
=============
Version 6.10.0 - 18707
	Fixed - after installing the Q-Logic driver, ASM was unable to discover the ARC driver. The reason was, ASM scan for the SCSI port number only up to 15 to discover ARC driver. The ARC driver was assigned a port number greater than 15 (increased the port scan up to 32 to resolve this issue).

Version 6.10.0 - 17557
	Fixed - Cannot see 2 LUNs with a SGXPCIESAS-R-EXT-Z card on J4400.
	Fixed - Sun RAID Manager: Selection time out when the ready drive is removed and inserted back.
	Fixed - Sun RAID Manager: JAVA Null Pointer Exception Error when creating Raid Volume.

Version 6.10.0 - 17551
	Fixed - PCI Bus/Dev/Fun was not correctly provided by SDK.

Version 6.10.0 - 17544
	Fixed - Adptec SDK failed to update the Drive FW under Windows.

Version 6.10.0 - 17537
	Included SDK for Windows, Linux and Solaris.
	Fixed - Displays incorrect PCI Bus/Dev/Fun/Slot numbers.

Version 6.10.0 - 17536
	Fixed - issue with Sun RAID Manager that was not showing the capacity of 1.5 TB drives. 

Version 6.10.0 - 17532
	Fixed - Sun RAID Manager RaidMan.jar (StorAgnt) interruptes IO every 10 min. affecting performance
	Fixed - Adaptec Storage Agent fails to start at boot when /opt is a mounted filesystem

Version 6.10.0 - 17523
	Fixed - Sun RAID Manager Reports RAID device degraded even after recovery of failed disk rebuild is completed

Version 6.10.0 - 17509
	Included the Latest build of Sun RAID Manager from the channel stream which includes
	¡¤	IPv6 support
	¡¤	Sun RAID Manager DAS agent autodiscovery	
	¡¤	Browser-based embedded help
	¡¤	W2K8 Server support
	¡¤	ARC: RAID-6
	¡¤	ARC: 256 drives
	¡¤	ARC: global background task priority

*Third-party trademarks are the property of their respective owners.
