================================================================================
Intel(R) Server Board S5000PSL and S5000XSL Firmware Update Package for 
Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility
================================================================================
INTEL Enterprise Products and Services Division
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : May 17, 2010
TO      : Intel(R) Server Board S5000PSL and S5000XSL customers
SUBJECT : Release Notes for system software update package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : S5000.86B.14.00.0099.03092010   March 9, 2010
BMC    : v00.66
FRUSDR : 48
================================================================================
                       Support Platform and Dependency
================================================================================
Intel(R) Server Platform S5000PSL and S5000XSL Processors supported:   
Intel(R) Xeon(R) Processor 5000 series w/ 533Mhz/667Mhz/1066Mhz FSB
Intel(R) Xeon(R) Processor 5100 series w/ 1066Mhz/1333Mhz FSB
Intel(R) Xeon(R) Processor 5200 series w/ 1066Mhz/1333Mhz FSB
Intel(R) Xeon(R) Processor 5300 series w/ 1066Mhz/1333Mhz FSB
Intel(R) Xeon(R) Processor 5400 series w/ 1066Mhz/1333Mhz FSB
    
Microcode update versions:
CPUID   Version Status  
0F64h   02      Production
0F65h   08      Production
06F6h   CD      Production 
06F7h   69      Production 
06FBh   B7      Production 
10676   60C     Production
1067A   A07     Production

On-Board Component Option ROM Versions:
ATI RN50 VGA    	: BK-ATI YJ20234a VER008.005.023.000	 
PXE Ver.        	: Intel(R) Boot Agent GE v1.2.45
ESB2 Option ROM 	: v A_02151557I
ESB2 AHCI Option ROM	: iSrc 1.08 09252006
Memory Reference Code Version:  1.32

Dependency:
EEPROM v03.01
HSC V2.14/2.12

Note: For Intel(R) Server Platform SC5400RA, you may encounter errors when you 
update BIOS/BMC/FRUSDR using this package via OFU or IDA. If errors occur, please 
use DOS SUP package to do System Firmware Update instead.
================================================================================
                  System Firmware Update Package Usage Instructions                   
================================================================================
This package can be updated using one of the following methods:
 - Intel(R) Deployment Assistant
 - Windows or Linux operating system using Intel(R) One-boot Flash Update (OFU)
   V9.70 Build4 or later)

Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD image from support.intel.com

User can use IDA CD to update system firmware by the following steps:
- Boot server with IDA CD
- Click "Get System Updates" Button at IDA home page
- IDA has three options to get system firmware update package

  . From support.intel.com
    IDA can automatically download system firmware update package from support.intel.com. 
    Server should have valid Internet connection. 
    User can follow the promps on IDA GUI to enter local server IP setting and 
    Internet proxy configuration.
    Select "Next" button to start firmware download and update process.
    
  . From my network
    IDA can access system firmware update package from a Windows share folder on LAN.
    User needs to download system firmware update package from support.intel.com
    and copy to a Windows share folder first.
    Follow the promps on IDA GUI to enter local server IP setting / 
    Windows* file server name / Windows* account name and its password.
    Find the system firmware update package in the Windows share folder from the
    IDA pop-up window.
    Select "Next" button to start firmware update process.
          
  . From USB Disk on Key or Hard Disk
    IDA can load system firmware update package from USB storage device.
    User needs to download system firmware update package from support.intel.com
    and copy it to a USB Disk on Key and insert it into server USB port.
    Select option "From USB Disk on key or Hard Disk" and select "Browse" button.
    Select system firmware update package ZIP file in the IDA pop-up window.
    Select "Next" to start firmware update.
    
  Note: System Firmware Update Package is in a .ZIP file format, no need to unzip,
        directly copy the .ZIP file to Windows folder or USB Disk on Key.

Intel(R) One-boot Flash Update (OFU)

To update from Windows and Linux or operating systems using the Intel(R) One Boot
Flash Update Utility

Intel(R) One boot Flash Update utility can be downloaded from support.intel.com
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows and Linux. Please refer to Intel OFU user guide for the details of 
installation and usage.

User can use OFU to update system firmware by the following steps:
- Install OFU on Windows or Linux system
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to a folder in Windows or Linux system
- Run the following command in Windows command line / Linux terminal window to 
  start firmware update process:
  <OFU install folder name>:\ flashupdt -u  <package folder name>\flashupdt.cfg
================================================================================
                         BIOS Changes since release R0098
================================================================================
Issues Fixed:
- Boot order issue when RMM2 is installed.
================================================================================
                        BMC Changes since release BMC00.65
================================================================================
Issues Fixed:
N/A
================================================================================
                      FRUSDR Changes since release FRUSDR48
================================================================================    
Issues Fixed:
N/A
================================================================================
                           LEGAL INFORMATION
================================================================================

Information in this document is provided in connection with Intel Products
and for the purpose of supporting Intel developed server boards and systems.
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation 
may have patents or pending patent applications, trademarks, copyrights, or
other intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2010 Intel Corporation.
================================================================================

[END OF RELEASE NOTES]