			HELP File for Platform Confidence Test

Version 1.1 of the EFI Platform Confidence Test

QUICK TEST 
 Quick test is designed to check the core components of the system;
 CPU, Memory,and RTC to ensure they are functioning properly. 
 Test time is between 2 and 5 minutes, depending on the amount memory.

 The test modules that are run during Quick Test:

 CACHE			RTC		IOH	
 CPU			Memory 		QPI
	

COMPREHENSIVE TEST 
 Comprehensive test performs a thorough test of the motherboard is a system.
 Test time is between 8 and 12 minutes, depending upon the amount memory.

 The test modules that are run during Comprehensive Test:

 CPU			Cache 
 Graphics		Memory
 KEYBOARD		IOH
 Real Time Clock	PCI Bus (PCI, PCIX, PCIe)
 Universal Serial Bus	Super I/O 
 SAS			ICHx			
 Hard Disks		NIC
 BMC			QPI
 HSC			RMM3


COMPREHENSIVE TEST With Continuous Looping 
 This is the same test listed above and will run until operator interrupts
 test cycle. To stop the test; press <F10>, system will transfer to 
 test menu screen with passed/failed displayed with total loops.

 Run time for the Comprehensive Test with continuous looping is between 
 8 and 15 minutes per pass, depending upon the amount memory that is 
 installed.

DISPLAY HELP TEXT 

 Display this help text file.

EXIT 

 Exit to EFI Shell.

To stop the testing at any time and return to test main menu; press <F10>.
