* 15 Jul 97 *

Q: Problem about install PNP sound blaster card?

A: Plug and play feature of WIN95 always set the sound card's IRQ/DMA 
   number to where our sound driver detection program couldn't be 
   located.
   In order to make a fine detection, please change the IRQ to 5 or 
   below 7 and DMA to 1 if possible.
   User can manual change it by right click the 'My Computer', open
   the sound driver's property, the option can be found on the resource
   tab.
