plugin_ctrl: unmapped=1, biosdev=1, speaker=1, extfpuirq=1
config_interface: textconfig
display_library: x
memory: host=32, guest=32
romimage: file="BIOS-bochs-latest"
vgaromimage: file="VGABIOS-lgpl-latest"
boot: c
floppy_bootsig_check: disabled=1
floppya: 1_44="boot.img", status=inserted
ata0: enabled=1, ioaddr1=0x1f0, ioaddr2=0x3f0, irq=14
ata0-master: type=disk, path="hdd.img", mode=flat, cylinders=1015, heads=16, spt=63
ata1: enabled=0, ioaddr1=0x170, ioaddr2=0x370, irq=15
ata2: enabled=0
ata3: enabled=0
parport1: enabled=0
parport2: enabled=0
com1: enabled=0
com2: enabled=0
com3: enabled=0
com4: enabled=0
usb_uhci: enabled=0
usb_ohci: enabled=0
usb_xhci: enabled=0
pci: enabled=0
vga: extension=vbe, update_freq=5
cpu: count=1, ips=4000000, model=bx_generic, reset_on_triple_fault=1, cpuid_limit_winnt=0
print_timestamps: enabled=0
port_e9_hack: enabled=0
private_colormap: enabled=0
clock: sync=none, time0=631148400
# no cmosimage
ne2k: enabled=0
pnic: enabled=0
sb16: enabled=0
es1370: enabled=0
# no loader
log: -
logprefix: %t%e%d
panic: action=ask
error: action=ignore
info: action=ignore
debug: action=ignore
keyboard_type: mf
keyboard_serial_delay: 250
keyboard_paste_delay: 100000
keyboard_mapping: enabled=0, map=
user_shortcut: keys=none
mouse: enabled=0, type=ps2, toggle=ctrl+mbutton
