Messages

Echo Chat
Echoed? Yes

Groups: 3
Symmetric Key (Gemini Encryption Key)
{
0 - 0000 (Base-64)
EOL
1 - Message (Base-64)
}
EOL
{
0 - Keyed (Gemini Hash Key) SHA-512 Message Code (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Groups: 4
Public Key
{
0 - 0000 (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key (Base-64)
EOL
3 - Symmetric Algorithm (Base-64)
}
EOL
Symmetric Key
{
0 - Dispatcher's SHA-512 Hash (Base-64)
EOL
1 - Name (Base-64)
EOL
2 - Message (Base-64)
EOL
3 - Sequence Number (Base-64)
EOL
4 - UTC Date (Base-64)
EOL
5 - Signature (Base-64)
}
EOL
{
0 - Keyed SHA-512 Message Code of the Second Group (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Echo Call
Echoed? Yes

Groups: 4
Public Key
{
0 - 0000(a | c) (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key (Base-64)
EOL
3 - Symmetric Algorithm (Base-64)
}
EOL
Symmetric Key
{
0 - Dispatcher's SHA-512 Hash (Base-64)
EOL
1 - Gemini Encryption Key (Base-64)
EOL
2 - Gemini Hash Key (Base-64)
EOL
3 - Timestamp (Base-64)
EOL
4 - Signature (Base-64)
}
EOL
{
0 - Keyed SHA-512 Message Code of the Second Group (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Groups: 3
Gemini Encryption Key
{
0 - 0000b (Base-64)
EOL
1 - Dispatcher's SHA-512 Hash (Base-64)
EOL
2 - Gemini Encryption Key (Base-64)
EOL
3 - Gemini Hash Key (Base-64)
EOL
4 - Timestamp (Base-64)
EOL
5 - Signature (Base-64)
}
EOL
{
0 - Keyed (Gemini Hash Key) SHA-512 Message Code (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Echo Mail
Echoed? Yes

Groups: 7
Public Key
{
0 - 0001a (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key 1 (Base-64)
EOL
3 - Symmetric Algorithm (Base64)
}
EOL
Symmetric Key
{
0 - Dispatcher's SHA-512 Hash (Base-64)
EOL
1 - Recipient's SHA-512 Hash (Base-64)
EOL
2 - Signature (Base-64)
}
EOL
Public Key
{
0 - 0001b (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key 2 (Base-64)
EOL
3 - Symmetric Algorithm (Base-64)
}
EOL
Symmetric Key
{
0 - Dispatcher's SHA-512 Hash (Base-64)
EOL
1 - Dispatcher's Name (Optional Gold Bug) (Base-64)
EOL
2 - Subject (Optional Gold Bug) (Base-64)
EOL
3 - Message (Optional Gold Bug) (Base-64)
EOL
4 - Attachment (Optional Gold Bug) (Base-64)
EOL
5 - Attachment Name (Optional Gold Bug) (Base-64)
EOL
6 - Signature (Optional Gold Bug) (Base-64)
EOL
7 - Gold Bug Used? (Base-64)
}
EOL
{
0 - Keyed 2 SHA-512 Message Code of the Fourth Group (Base-64)
}
EOL
{
0 - Keyed 1 SHA-512 Message Code of the Second Group (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Groups: 4, 7
Public Key
{
0 - 0001b (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key (Base-64)
EOL
3 - Symmetric Algorithm (Base-64)
}
EOL
Symmetric Key
{
0 - Dispatcher's SHA-512 Hash (Base-64)
EOL
1 - Dispatcher's Name (Optional Gold Bug) (Base-64)
EOL
2 - Subject (Optional Gold Bug) (Base-64)
EOL
3 - Message (Optional Gold Bug) (Base-64)
EOL
4 - Attachment (Optional Gold Bug) (Base-64)
EOL
5 - Attachment Name (Optional Gold Bug) (Base-64)
EOL
6 - Signature (Optional Gold Bug) (Base-64)
EOL
7 - Gold Bug Used? (Base-64)
}
EOL
{
0 - Keyed SHA-512 Message Code of the Second Group (Base-64)
}
EOL
{
0 - Optional Random Message (Base-64)
}
EOL
{
0 - Optional Keyed (Institution Hash Key)
    Message Code of the Optional Random Message and the Recipient's Public
    Key (Base-64)
}
EOL
{
0 - Optional Keyed (Institution Hash Key)
    Message Code of the Preceding Five Groups (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Retrieve Mail
Echoed? Yes

Groups: 4
Public Key
{
0 - 0002a (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key (Base-64)
EOL
3 - Symmetric Algorithm (Base-64)
}
EOL
Symmetric Key
{
0 - Requester's SHA-512 Hash (Base-64)
EOL
1 - Random Message (Base-64)
EOL
2 - Timestamp (Base-64)
EOL
3 - Signature (Base-64)
}
EOL
{
0 - Keyed SHA-512 Message Code of the Second Group (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Groups: 3
Symmetric Key (Institution Encryption Key)
{
0 - 0002b (Base-64)
EOL
1 - Random Message (Base-64)
EOL
2 - Keyed (Institution Hash Key) Message Code of the Random Message
    and the Requester's Public Key (Base-64)
EOL
3 - Random Message (Base-64)
EOL
4 - Timestamp (Base-64)
EOL
5 - Signature (Base-64)
}
EOL
{
0 - Keyed (Institution Hash Key) Message Code (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Key Exchange
Echoed? No

Message Type ("0011" or "0012")
0 - Key Type (Base-64)
EOL
1 - Dispatcher's Name (Base-64)
EOL
2 - Dispatcher's Public Key (Base-64)
EOL
3 - Dispatcher's Public Key Signature (Base-64)
EOL
4 - Dispatcher's Signature Public Key (Base-64)
EOL
5 - Dispatcher's Signature Public Key Signature (Base-64)

Participant Status
Echoed? Yes

Groups: 3
Symmetric Key (Gemini Encryption Key)
{
0 - 0013 (Base-64)
EOL
1 - Message (Base-64)
}
EOL
{
0 - Keyed (Gemini Hash Key) SHA-512 Message Code (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Groups: 4
Public Key
{
0 - 0013 (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key (Base-64)
EOL
3 - Symmetric Algorithm (Base-64)
}
EOL
Symmetric Key
{
0 - Dispatcher's SHA-512 Hash (Base-64)
EOL
1 - Name (Base-64)
EOL
2 - Status (Base-64)
EOL
3 - UTC Date (Base-64)
EOL
4 - Signature (Base-64)
}
EOL
{
0 - Keyed SHA-512 Message Code of the Second Group (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

UUID Exchange
Echoed? No

Message Type ("0014")
UUID (Base-64)

Echo Listener Publication
Echoed? Yes

Message Type ("0030")
0 - IP Address (Base-64)
EOL
1 - Port (Base-64)
EOL
2 - Scope ID (Base-64)
EOL
3 - Transport (Base-64)
EOL
4 - Orientation (Base-64)

Echo Buzz
Echoed? Yes

Groups: 2
Symmetric Key
{
0 - 0040a (Base-64)
EOL
1 - Name (Base-64)
EOL
2 - ID (Base-64)
}
EOL
{
0 - Keyed Message Code (Base-64)
}

Groups: 2
Symmetric Key
{
0 - 0040b (Base-64)
EOL
1 - Name (Base-64)
EOL
2 - ID (Base-64)
EOL
3 - Message (Base-64)
}
EOL
{
0 - Keyed Message Code (Base-64)
}

Account Authentication
Echoed? No

Message Type ("0050") (Client Request)
0 - Keyed SHA-512 Hash (Base-64)
EOL
1 - Random Data (Base-64)

Message Type ("0051") (Server Response)
0 - Keyed SHA-512 Hash (Base-64)
EOL
1 - Random Data (Base-64)

Message Type ("0052") (Server Authentication Request)
0 (Base-64)

StarBeam
Echoed? Yes

Groups: 3
Symmetric Key
{
Optional Nova AES-256
{
0 - 0060 (Base-64)
EOL
1 - File Name (Base-64)
EOL
2 - Pulse Offset (Base-64)
EOL
3 - Data Size (Base-64)
EOL
4 - Total Size (Base-64)
EOL
5 - Pulse Data (Base-64)
EOL
6 - Pulse Size (Base-64)
}
Optional Nova SHA-512
{
0 - Keyed Message Code (Base-64)
}
}
EOL
{
0 - Keyed SHA-512 Message Code (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Buzz Magnet Share
Echoed? No

Message Type ("0065")
0 - Buzz Magnet (Base-64)

Message of the Day
Echoed? No

Message Type ("0070")
MOTD (Base-64)

Request Weather Station's Public Keys
Echoed? No

Message Type ("0080")
0 (Base-64)

Request Weather Data
Echoed? Yes

Groups: 4
Public Key
{
0 - 0081 (Base-64)
EOL
1 - Encryption Symmetric Key (Base-64)
EOL
2 - SHA-512 Hash Key (Base-64)
EOL
3 - Symmetric Algorithm (Base-64)
}
EOL
Symmetric Key
{
0 - URL (Base-64)
EOL
1 - Location Attributes (Base-64)
}
EOL
{
0 - Keyed SHA-512 Message Code of the Second Group (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}

Receive Weather Data
Echoed? Yes

Groups: 3
Symmetric Key
{
0 - 0082 (Base-64)
EOL
1 - RSS (Base-64)
}
EOL
{
0 - Keyed SHA-512 Message Code (Base-64)
}
EOL
{
0 - Keyed (Adaptive Echo Hash Key) Message Code of the
    Preceding Data and Encrypted Timestamp,
    Encrypted Timestamp (Base-64)
}
