M=Nodule
D=Description
C=compile time dependend
R=runtime dependend
I=Info
S=Status
P=processing modes

M: import_ac3.c
D: (audio) AC3
C: none
R: none
S: +
I: decodes AC3 audio from MPEG program streams or raw streams.
P: audio - PCM AC3, video - none

M: import_af6.c
D: (video) Win32 dll | (audio) PCM
C: avifile
R: avifile, win32codecs
S: o
I: interface to avifile library supported codecs and file formats.
P: audio - PCM, video - RGB YUV

M: import_avi.c
D: (video) * | (audio) *
C: none
R: none
S: +
I: RGB/PCM from RIFF AVI files.
P: audio - RAW (pass-through) PCM, video - RAW (pass-through) RGB YUV YUV420

M: import_bktr.c
D: (video) bktr
C: none
R: none
S: +
I: grabs video frames from bktr(4) devices on BSD systems
P: audio - none, video - RGB YUV YUV420

M: import_divx.c
D: (video) DivX;-)/XviD/OpenDivX/DivX 4.xx/5.xx
C: none
R: libdivxencode
S: -
I: decoding support for AVI-files with DivX, OpendivX, DivX 4.xx/5.xx, XviD video using the DivX codec.
P: audio - none, video - RAW (pass-through) RGB YUV

M: import_dv.c
D: (video) DV | (audio) PCM
C: none
R: none
S: +
I: Digital Video and PCM audio from RIFF AVI-files or raw streams.
P: audio - PCM, video - RAW (pass-through) RGB YUV DV YUV420

M: import_dvd.c
D: (video) DVD | (audio) MPEG/AC3/PCM
C: libdvdread
R: none
S: +
I: on-the-fly DVD transcoding.
P: audio - PCM AC3, video - RGB YUV

M: import_ffbin.c
D: (video) rendered by ffmpeg binary | (audio) rendered by ffmpeg binary
C: none
R: ffmpeg binary
S: +
I: audio and video decoded by the ffmpeg binary.
P: processing modes: audio - PCM, video - RAW (pass-through) RGB YUV

M: import_ffmpeg.c
D: (video) FFmpeg: MSMPEG/MPEG/MJPEG
C: none
R: none
S: +
I: interface to ffmpeg library supported video codecs and file formats
P: audio - none, video - RAW (pass-through) RGB YUV

M: import_fraps.c
D: (video) * 
C: none
R: none
S: -
I: decodes fraps, FPS1, a packed form of YUV420
P: audio - none, video - YUV

M: import_im.c
D: (video) RGB
C: ImageMagick
R: ImageMagick
S: o
I: interface to ImageMagick library supported picture codecs and file formats for making animations. Reads images with a counter pattern.
P: audio - none, video - RAW (pass-through) RGB

M: import_imlist.c
D: (video) RGB
C: ImageMagick
R: ImageMagick
S: o
I: interface to ImageMagick library supported picture codecs and file formats for making animations. Reads images from a list.
P: audio - RAW (pass-through), video - RAW (pass-through) RGB

M: import_lav.c
D: (video) LAV | (audio) WAVE
C: none
R: mjpegtools
S: +
I: interface to mjpegtools (YUV4MPEG) streams produced by lav2yuv and lav2wav.
P: audio - PCM, video - RGB YUV

M: import_lve.c
D: (video/audio) MPEG/VOB/LVE
C: liblve
R: none
S: o
I: imports video from an LVE edit list
P: audio - PCM, video - YUV

M: import_lzo.c
D: (video) LZO
C: lzo
R: none
S: +
I: imports AVI-files with LZO loss-less compression for video.
P: audio - RAW (pass-through) PCM, video - RAW (pass-through) RGB YUV

M: import_mov.c
D: (video) * | (audio) *
C: libquicktime
R: none
S: +
I: Quicktime file format, audio/video codecs supported by quicktime4linux.
P: audio - PCM, video - RAW (pass-through) RGB YUV

M: import_mp3.c
D: (audio) MPEG
C: none
R: none
S: +
I: MPEG audio from program streams or raw streams.
P: audio - PCM, video - none

M: import_mpeg2.c
D: (video) MPEG2
C: none
R: none
S: +
I: video track from MPEG program streams or raw streams, extracted and decoded by mpeg2dec.
P: audio - none, video - RAW (pass-through) RGB YUV

M: import_mpeg3.c
D: (video) MPEG2 | (audio) MPEG/AC3/PCM
C: libmpeg3
R: libmpeg3
S: o
I: video track from MPEG program streams or raw streams extracted and decoded by libmpeg3.
P: audio - RAW (pass-through) PCM, video - RGB YUV

M: import_mplayer.c
D: (video) rendered by mplayer | (audio) rendered by mplayer
C: none
R: mplayer
S: o
I: interface to Mplayer for decoding unsupported codecs, exotic file formats or more ore less broken sources.
P: audio - PCM, video - RAW (pass-through) RGB YUV

M: import_net.c
D: (video) RGB/YUV | (audio) PCM
C: none
R: none
S: -
I: read raw video/audio streams from sockets.
P: audio - PCM, video - RGB YUV

M: import_null.c
D: (video) null | (audio) null
C: none
R: none
S: o
I: dummy module, reads from /dev/zero.
P: audio - none, video - none

M: import_nuv.c
D: (video) YUV | (audio) PCM
C: none
R: none
S: o
I: interface to NuppelVideo file format.
P: audio - PCM, video - YUV

M: import_nvrec.c
D: (video) nvrec | (audio) nvrec
C: none
R: nvrec
S: o
I: interface to NVrec video recorder program.
P: audio - PCM, video - YUV

M: import_ogg.c
D: (video) all | (audio) Ogg Vorbis
C: none
R: none
S: +
I: decodes Ogg Vorbis audio streams.
P: audio - RAW (pass-through) PCM, video - RAW (pass-through) RGB YUV

M: import_pvn.c
D: (video) PVN
C: none
R: none
S: o
I: imports video in the PVN format.
P: audio - RAW (pass-through), video - RAW (pass-through) RGB

M: import_raw.c
D: (video) RGB/YUV | (audio) PCM
C: none
R: none
S: o
I: RGB/PCM from RIFF AVI/WAVE files or raw streams.
P: audio - PCM, video - RGB YUV YUV420

M: import_rawlist.c
D: (video) YUV/RGB raw frames
C: none
R: none
S: o
I: reads images from a list. Native support for raw image formats only.
P: audio - RAW (pass-through), video - RGB YUV YUV420

M: import_sh.c
D: (video) * | (audio) *
C: none
R: none
S: o
I: runs commands and reads from stdin.
P: audio - RAW (pass-through) PCM AC3, video - RAW (pass-through) RGB YUV YUV420

M: import_sunau.c
D: (audio) pcm
C: none
R: none
S: +
I: grabs raw PCM audio from audio(4) devices on some BSD systems
P: audio - PCM, video - none

M: import_v4l.c
D: (video) v4l | (audio) PCM
C: none
R: none
S: o
I: interface for grabbing sound/video from v4l devices on linux systems.
P: audio - PCM, video - RGB YUV

M: import_v4l2.c
D: (video) v4l2 | (audio) pcm
C: none
R: none
S: +
I: interface for grabbing sound/video from v4l2 devices on linux systems. prefered over import_v4l.
P: audio - PCM, video - RGB YUV YUV420

M: import_vdrac3.c
D: (audio) VDR-AC3
C: none
R: none
S: o
I: AC3 audio with invalid AC3 audio stream header from MPEG streams produced by digital capture cards.
P: audio - PCM AC3, video - none

M: import_vnc.c
D: (video) VNC
C: none
R: vncrec
S: o
I: imports video from the vncrec program.
P: audio - none, video - RAW (pass-through) RGB YUV

M: import_vob.c
D: (video) MPEG-2 | (audio) MPEG/AC3/PCM | (subtitle)
C: none
R: none
S: +
I: MPEG/AC3 program streams in VOB files (found on unencrypted/ripped DVDs).
P: audio - PCM AC3, video - RAW (pass-through) RGB YUV

M: import_xml.c
D: (video) * | (audio) *
C: libxml2
R: libxml2
S: o
I: interface to XML files with file listing and frame range produced by kino.
P: audio - RAW (pass-through) PCM, video - RAW (pass-through) RGB YUV DV

M: import_xvid.c
D: (video) XviD/OpenDivX/DivX 4.xx/5.xx
C: none
R: libxvidcore
S: o
I: decoding support for AVI-files with DivX, OpendivX, DivX 4.xx/5.xx, XviD video using the XviD codec.
P: audio - none, video - RAW (pass-through) RGB YUV

M: import_yuv.c
D: (video) YUV files 
C: none
R: none
S: o
I: imports directories of files containing single YUV frames.
P: audio - none, video - YUV

M: import_yuv4mpeg.c
D: (video) YUV4MPEGx | (audio) WAVE
C: none
R: none
S: +
I: YUV from video streams produced by mjpegtools (YUV4MPEG) and RIFF WAVE pcm audio.
P: audio - PCM, video - RGB YUV
