#

Manual Reference Pages - debugsh (1)

### NAME

> debugsh - Simple debugging console for a Palm Handheld device [deprecated].

### CONTENTS

> Section
> Synopsis
> Description
> Usage
> Author
> Copyright

### SECTION

> pilot-link: Tools

### SYNOPSIS

> debugsh /dev/tty<0..n>

### DESCRIPTION

> debugsh is a commandline interface to the Palm debug monitor. Use device file /dev/tty<0..n> to communicate with the Palm handheld. If this is not specified, debugsh will output a simple usage help message.

### SHELL COMMANDS

> coldboot

> > Restart your Palm

> reboot

> > Restart your Palm

> numdb

> > Returns the number of databases on the PDA card.

> dbinfo

> > Returns the names of databases on the Palm.

> quit

> > Quits the debug shell.

### USAGE

> The program will connect to your Palm handheld and give the user an interactive prompt (a "shell") for executing debugging commands.

### AUTHOR

> This manual page was written by Ludovic Rousseau rousseau@debian.org for the Debian GNU/Linux system.

> Updated for pilot-link 0.12 by Neil Williams linux@codehelp.co.uk

### REPORTING BUGS

> Report bugs at: http://bugs.pilot-link.org

### COPYRIGHT

> This program is free software; you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation; either version 2 of the License, or (at your option) any later version.

> This program is distributed in the hope that it will be useful, but WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the GNU General Public License for more details.

> You should have received a copy of the GNU General Public License along with this program; if not, write to the Free Software Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA

### SEE ALSO

> pilot-link(7)

pilot-link 0.12.0-pre4 | debugsh (1) | Copyright 1996-2005 FSF

Generated by manServer 1.07 from e:\usr\local\palm\man\man1\debugsh.1 using man macros.