## minss, minsd, minps, minpd - minimum

    dest = min(source)

The minss, minsd, minps, and minpd instructions computes the minimum of the source and the destination and store the result(s) in the destination operand. There are also vminss, vminsd, vminps, and vminpd on CPUs with AVX instructions which can compute multiple values at once. Behaviorally these instructions are similar to the various add instructions should you wish to see more details.

            minss   xmm0, xmm1          ; xmm0 gets 32 bit min of xmm1
            minsd   xmm0, [x]           ; xmm0 gets 64 bit min of x
            minps   xmm0, [rdi]         ; xmm0 gets 4 32 bit mins of [rdi]
            minpd   xmm0, [x+4*rcx]     ; xmm0 gets 2 64 bit mins of array x
            vminps  xmm3, xmm4, xmm15   ; xmm3 gets 4 32 bit mins of xmm4 & xmm15
            vminps  ymm3, ymm4, ymm15   ; ymm3 gets 8 32 bit mins of ymm4 & ymm15
            vminpd  ymm3, ymm5, [x]     ; ymm3 gets 4 64 bit mins of ymm5 & array x

### flags: none