            segment .data
    coeff   dq      1.0, 2.0, 3.0, 4.0
    x       dq      2.0

            segment .text
            global  main, horner
    main:
            push    rbp
            mov     rbp, rsp
    	sub	rsp, 32
            lea     rdi, [coeff]
            movsd   xmm0, [x]
            mov     esi, 3
            call    horner
            xor     eax, eax
            leave
            ret

    horner: movsd   xmm1, xmm0          ; use xmm1 as x
            movsd   xmm0, [rdi+rsi*8]   ; accumulator for b_k
            cmp     esi, 0              ; is the degree 0?
            jz      done
            more:   sub     esi, 1
            mulsd   xmm0, xmm1          ; b_k * x
            addsd   xmm0, [rdi+rsi*8]   ; add p_k
            jnz     more
    done:   ret