SAMPLES directory contents:
---------------------------

BASIC_IO  - Sample skeleton driver for a simple ISA card with 
            access to the IO ports.

INT_IO    - Sample skeleton driver for an ISA card. The driver 
            implements IO port access and interrupt handler 
            installation.

PCI_DIAG  - Sample skeleton driver for a PCI card. The driver 
            implements PCI detection, accessing memory mapped 
            ranges on the card, and interrupt handler installation.

PCI_DUMP  - A utility for getting a dump of all the PCI 
            configuration registers of the PCI cards installed.

PCI_SCAN  - A utility for getting a list of the PCI cards installed 
            and the resources allocated for each one of them (memory 
            ranges, IO ranges and interrupts).

PCI_DMA   - Demonstrates programing a PCI device for Bus master transfers.

WDDEBUG   - A utility that turns WinDriver's debug mode on and off,
            and allows viewing the debug messages from the kernel.
            When in debug mode, every IO and memory transfer command
            are checked, making sure they fit in with the card's 
            registered resources. 
            If an illegal command is given, WinDriver
            will ignore the command and show a warning message on
            screen. Debug mode slows down transfer operations, 
            therefore it should be used only in the development 
            process. Running this command without the "on" / "off" 
            parameter will print the version of WinDriver installed.

WDREG     - Registers/Unregisters WinDriver in the Windows registery. 
            To install WinDriver on a new computer, 
            copy WINDRVR.VXD file to C:\WIN95\SYSTEM\VMM32 (Win95), or
            copy WINDRVR.SYS file to C:\WINNT\SYSTEM32\DRIVERS (WinNT). 
            After copying WinDriver to the drivers directory, add 
            WinDriver to the list of Device Drivers Windows loads on 
            boot by running "WDREG.EXE install". To install WinDriver 
            from within your own application, add the "wdreg" source 
            to your own installation code.

ISAPNP_SCAN  - A utility for getting a list of the ISA PnP cards 
            installed and the resources allocated for each one 
            of them (memory ranges, IO ranges and interrupts). 

SPEAKER   - Demonstrates accessing IO ports. This sample programs the 
            motherboard's timer that is connected to the speaker, to
            generate tones.

SPEAKER_GUI - A Win32 GUI application that demonstrates using WinDriver 
            in a GUI application. This is the GUI version of the speaker
            sample.

CMOS      - This sample reads the CMOS date and time.

SHARED    - Shared source code used by sample applications.

