| Version 5.4
Introduction
Installation
SysAdmin
Network
Objects
Storage
E-mail
Real-Time
Access
Services
Directory
Clusters
Applications
Miscellaneous
Licensing
WebMail
Pronto!
PBX
Overview | Call Control | Voicemail | Services | PBX Center | Conference
# PBX: Voicemail Launching VoiceMail Recording Messages Composing Voice Messages Accessing Services Calling Home Alternative Address Your Account can be configured to start the `voicemail` application when you are busy, not available, or not answering. This section describes the `voicemail` application and its features.

## Launching VoiceMail

To specify when the `voicemail` application should accept your incoming calls, open the Call Control WebUser Interface page.

The voicemail application can be configured to start when:

- your Account has no registered device
- none of your devices is picked up after certain "ringing" (alerting) time
- all your devices have rejected the call
- you have pressed the DND (Do Not Disturb) button on any of your registered devices
- the caller is the Blocked list
- the current time is outside your working hours
- your current Presence status is set to the pre-defined value (busy, away, etc.)

A Router Default Record starts an Account `voicemail` application when a `*nnn` number is dialed, where nnn is an Account numeric alias.
This feature can be used by a receptionist to transfer or redirect certain calls directly to the callee's voicemail.

## Recording Messages

The stock `voicemail` application performs the following operations:

- The application plays a greeting. It can be the standard greeting or your custom greeting.
- The application allows a caller to record a voice message, to review that message, to re-record the message, to mark the message as urgent, or to cancel the recorded message.
- The application allows a caller to listen to custom greeting (private announcements).
  The caller should press `6` and provide the correct announcement PIN.
- The application allows a caller to join your personal conference. The caller should press `7` and provide your personal Conference PIN that you have set using the WebUser Interface.

## Composing Voice Messages

Voice Messages are composed as voice-type E-mails and mailed to your Account.

Your Account Queue/Mail Rules will be applied to the voice messages before they are stored in your INBOX.
If you E-mail client does not support voice-type E-mails, you will see voice messages as audio-file attachments. You can play these messages by opening these attachments.

## Accessing Services

You can use the `voicemail` application to start your `service` application when you cannot call from your own VoIP phone (for example, when you are calling from a PSTN phone via a gateway).

Press the `*` (star) symbol twice while listening to the greeting and/or the menu options. The application will ask you to enter your Access PIN. If the number is correct, the application switches you to the `service` application menu.

## Calling Home

You can use the WebUser Interface to configure your Home PSTN Number.

The voicemail application compares the local part of the caller address (the phone number) with the Home PSTN Number value. If the tail of the address matches the specified value, the application asks the caller to enter the Access PIN and then it switches to the `service` application.

Since the application checks only the address tail, you can specify your Home PSTN Number as a local number, or as a number without the country code.

## Alternative Number

You can use the WebUser Interface to configure the Alternative Number. If callers press the `9` button, they are transferred to the Alternative Number.
For example, you can specify the `pbx` or `operator` address with this setting, so the callers can transfer themselves to the company automatic or live attendant if they do not want to leave a voicemail for you.

CommuniGate® Pro Guide. Copyright © 1998-2012, Stalker Software, Inc.