
                  OS/2 PRINT SUBSYSTEM PRINTER DRIVER
                   FOR OS/2 WARP v2.11 AND ABOVE

                              IMPORTANT
                              ---------
    PLEASE READ THE FOLLOWING TERMS AND CONDITIONS. DOWNLOADING
    THE FIX THAT FOLLOWS, INDICATES YOUR ACCEPTANCE OF THE
    FOLLOWING TERMS AND CONDITIONS:

    - YOU MUST BE, AND YOU AGREE THAT YOU ARE, A PRIOR LICENSEE OF OS/2
      WARP 
    - YOU MAY MAKE COPIES OF THE OS/2 WARP SERVICE FIX EQUAL TO
      THE NUMBER OF LICENSED COPIES OF OS/2 WARP VERSIONS YOU POSSESS
    - YOU MAY ONLY USE THIS MAINTENANCE UPDATE PURPOSES
    - ALL OTHER TERMS AND CONDITIONS OF YOUR OS/2 WARP VERSION LICENSE
      AGREEMENT APPLY TO THIS SERVICE FIX; HOWEVER, THIS DOES NOT EXTEND ANY
      WARRANTY OUTLINED IN SUCH AGREEMENT.



PRINTER DRIVER LEVEL =   Epson OMNI4 Version 1
-----------------------------

FILES INCLUDED IN THIS ARE:
-----------------------------------
README       - INSTALLATION INSTRUCTIONS (THIS FILE)
EPOMNI4.DRV  - EPOMNI4 DRIVER
EPOMNI4.EA   - EPOMNI4 DRIVER EAs.
EPOMNI4.LST  - LIST OF EPSON DEVICES
EPIUMW40.DLL - EPSON DEVICE FILE 
EPIHMM40.DLL - EPSON DEVICE FILE 
EPUT001.DLL  - EPSON DEVICE FILE 
EPRS001.DLL  - EPSON DEVICE FILE 
EPIJ4S30.DLL - EPSON DEVICE FILE 
EPIJ4S3R.DLL - EPSON DEVICE FILE 
EPISRA4P.DLL - EPSON DEVICE FILE 
EPISRA5A.DLL - EPSON DEVICE FILE 
EPISRA5B.DLL - EPSON DEVICE FILE 
EPISRA5D.DLL - EPSON DEVICE FILE 

TO INSTALL THIS FIX PERFORM THE FOLLOWING STEPS :
-----------------------------------------------

 Use these printer drivers as you would your original printer driver


 - Unpack printer driver by executing epomni.exe in a directory of your
   choice
 - Open the printer object(s) and deselect all drivers you have
   acquired this fix for and select another driver file as default.
 - Close the printer object.
 - Reboot the system without letting any print jobs print.
 - Point to a printer object
 - Click Mouse Button 2
 - Select properties
 - Select the printer driver tab
 - Point to one of the printer driver objects
 - Click mouse button 2
 - Select the install printer driver
 - The "Install New Printer Driver" dialog will appear.
 - Select "Other OS/2 Printer Driver" and enter the drive and/or
   directory that you have put the driver files into for the install.
 - Press Refresh button to refresh the driver list that is installed on
   the diskette.
 - Select the driver to install and press Install button
 - Select OK to close the "Install New Printer Driver" dialog and
   select the correct driver for the print object
 - Close print object.
 ***
 - A Second Method of installing is to select the printer object in the source directory
 - Pick the printer object you want to install by dragging and droping onto the desktop.

You will now be ready to print using the driver.  If you need additional
help installing the printer driver, please refer to the on-line help
facility.

Note 2:
------
If you are in a network environment, we suggest that you match printer
driver levels between both the server and the requestors.

PRINTER DEVICES INCLUDED 
--------------------------------
Epson Stylus Color 670
Epson Stylus Color 680
Epson Stylus Color 777
Epson Stylus Color 880
Epson Stylus Color 980


The required files to use Stylus Color 670.
EPOMNI4.DRV
EPIUMW40.DLL
EPIHMM40.DLL
EPUT001.DLL
EPRS001.DLL
EPIJ4S30.DLL
EPISRA4P.DLL

The required files to use Stylus Color 680.
EPOMNI4.DRV
EPIUMW40.DLL
EPIHMM40.DLL
EPUT001.DLL
EPRS001.DLL
EPIJ4S3R.DLL
EPISRA5D.DLL

The required files to use Stylus Color 777.
EPOMNI4.DRV
EPIUMW40.DLL
EPIHMM40.DLL
EPUT001.DLL
EPRS001.DLL
EPIJ4S3R.DLL
EPISRA5D.DLL

The required files to use Stylus Color 880.
EPOMNI4.DRV
EPIUMW40.DLL
EPIHMM40.DLL
EPUT001.DLL
EPRS001.DLL
EPIJ4S3R.DLL
EPISRA5B.DLL

The required files to use Stylus Photo 980.
EPOMNI4.DRV
EPIUMW40.DLL
EPIHMM40.DLL
EPUT001.DLL
EPRS001.DLL
EPIJ4S30.DLL
EPISRA5D.DLL

