----------------------------------------------------------------------------
                   INSTALLATION  INSTRUCTIONS OS/2 V3.0 (WARP)

NOTE: The Installation Diskette 1 volume label must be "MAGIC 1".
Please use the diskcopy utility if backup diskettes are made.

NOTE: This procedure assumes you are installing from A: to C:  If this
is not the case make appropriate adjustments.

1.      Open OS/2 SYSTEM.

2.      Open COMMAND PROMPTS.

3.      Open an OS/2 WINDOW or OS/2 FULL SCREEN command session.

4.      Insert the NeoMagic -- MAGICGRAPH128/V/ZV/XD Installation diskette
        in drive A.

5.      From the OS/2 session type "A: [enter]".
        Then from the A: prompt type "setup c" [enter]

6.      From the DISPLAY DRIVER INSTALL window,
             select PRIMARY DISPLAY
             select OK.

7.      From the PRIMARY DISPLAY DRIVER LIST window,
             select NeoMagic -- MAGICGRAPH128/V/ZV/XD
             select OK.

8.      From the SOURCE DIRECTORY window,
             make sure source directory points to location of
                  installation diskette (use Change radio button
                  to select the proper drive, if necessary)
             select INSTALL

9.      After installation of files on Diskette 1 is complete,
             from the DISPLAY DRIVER INSTALL pop-up window,
             select OK

10.     Shut down by selecting the Shut down button on the Launch Pad,
        and reboot the system.

11.     If you want to change screen resolution then proceed with
        the appropriate Screen Resolution Modification instructions
        below.  (defaults to 640 x 480)

----------------------------------------------------------------------------
OS/2 3.0 (Warp) Resolution Modification

To change resolutions and pixel depths within the driver AFTER INSTALLATION,
take the following steps:

1.      Click your right mouse button on the OS/2 Desktop and select the
        entry "System Setup".  When the folder opens, double click on
        the SYSTEM icon.

2.      Select the Screen Resolution from among those listed, then close
        the System Settings Window by double clicking on the top-left
        corner.

(NOTE: you must shut-down using the Shut down radio button on the Launch
 pad, and re-boot before the change will actually take place)

