COMi Installation and Configuration

To install the Connect Tech DFLEX or Blue Heat COMi asynchronous serial device
driver, do one of the following:

Method One:

1. Open the OS/2 System folder

2. Open the Drives folder

3. Double click on the drive that contains the distribution diskette.

4. Double click on the INSTALL.EXE icon.

5. Once INSTALL is loaded, use the "Install..." menu item to setup the
   installation for your system requirements and transfer the required
   files to your system.

    Select "Installation | Install..."

6. Use the "Configuration | COMi..." menu item to configure the COMi 
   device driver. The configuration process has plenty of on-line help
   to help with setting up COMi.

7. Shutdown and re-boot your system.

Method Two:

1. Open an OS/2 command prompt session.

2. Make the disk drive containing the distribution diskette the default drive.

    Example:  [C:\]A: [ENTER)
              (assuming the distribution diskette is in drive A:)

3. Start INSTALL.EXE by typing INSTALL [ENTER]

4. Follow the instructions from item five, above.

Once installed, you may use INSTALL at any time to change the configuration
of the COMi device driver and any device controlled by COMi.  Any changes you
make will require a re-boot to take effect.

Your distribution diskette contains the file IOCTL.C.  IOCTL.C contains "C"
source code sample functions for most of the DosDevIOCtl functions defined for
Category One Asynchronous Serial Devices as defined in the "Physical Device
Driver Technical Reference".  A header file, IOCTL.H, is also included.

COMi and INSTALL are the property of OS/tools Incorporated and are
copyrighted (c) 1989-2002 by OS/tools Incorporated with all rights reserved.

These programs are licensed to you on a per machine basis.  One license is
required for each machine on which they are installed.

We know nothing and are responsible for nothing, except for any increased
productivity and/or pleasure brought about by the use of these programs.  This
is the only disclaimer you have to read.

For additional information about COMscope, COMspool, the COMi device
driver, or other OS/tools products please contact:

OS/tools Incorporated
7145 Yorktown Drive
Gilroy, CA 95020
Phone: (408)847-7487, FAX: (408)847-7480
Internet: e-mail: products@os-tools.com, URL: http://www.os-tools.com

For more information on products from Connect Tech please contact:  

Connect Tech Incorporated
727 Speedvale Avenue West
Guelph, Ontario, Canada  N1E 1E6
Phone (519)836-1219  FAX (519)836-4878 

OS/tools, COMscope, COMspool, COMsuite, and COMi are trademarks of 
OS/tools Incorporated.

OS/2 is a trademark of International Business Machines, Incorporated.

