COMi Quick Installation

To install the COMi asynchronous serial device driver do one of the following:

Method One:

 1. Open an OS/2 command prompt session.

 2. Make the disk drive containing the distribution diskette the default drive.

     Example:  [C:\]A: <ENTER>
               (assuming the distribution diskette is in drive A:)

 3. Start Quick Install by typing QINST <ENTER>

Method Two:

 1. Open the OS/2 System folder

 2. Open the Drives folder

 3. Double click on the drive that contains the distribution diskette.

 4. Double click on the QINST.EXE icon.

Quick Install transfers all required files, including a preconfigured 
initialization file for COMi, and creates desktop objects for the
COMi Users Guide and the COMi Configuration application.

Once installed, you may use The "COMi Configuration" object located in the 
"OStools Utilities" folder at any time to change the configuration of the COMi
device driver and any device controlled by COMi, though any changes you make
will require a re-boot to take effect.

COMi and Quick Install are the property of OS/tools Incorporated and are 
copyrighted (c) 1989-95 by OS/tools Incorporated with all rights reserved.

These programs are licensed to you on a per CPU basis.  One license is
required for each CPU on which they are installed.

We know nothing and are responsible for nothing, except for any increased
productivity and/or pleasure brought about by the use of these programs.  This
is the only disclaimer you have to read.

For additional information about SafePage, PageStar, QuickPage, COMscope,
COMspool, the COMi device driver, or other OS/tools products please contact:

OS/tools Incorporated
1685 Branham Lane Suite OS/2
San Jose, CA 95118-5226
(408)269-9411 FAX (408)269-9434
OR
E-mail to products@os-tools.com on the internet or to 70314,3235 on CompuServe.

OS/tools, SafePage, PageStar, QuickPage, OS/tools, COMscope, COMspool, and
COMi are trademarks of OS/tools Incorporated.

OS/2 is a trademark of International Business Machines, Incorporated.

