Appendix A. System Specifications
Prev |  | Next

## Appendix A. System Specifications

Table A-1 and Table A-2 provide technical specifications for the Origin2000 rack system.

Table A-1. Physical and Environmental Specifications

Parameter |  | Specification
--- | --- | ---
Dimensions |  |
Installed: | length width height | 39” (99 cm) 29” (74 cm) 73” (185 cm)
Shipping: | length width height | 81” (206 cm) 47” (120 cm) 49” (125 cm)
Weight: | minimum (empty rack) maximum (full rack) shipping (maximum) | 300 lbs (136 kg) 750 lbs (340 kg) 900 lbs (408 kg)
Floor Loading: | minimum maximum | 38 lb/ft2 (185 kg/m2) 95 lb/ft2 (466 kg/m2)
Air Temperature: | operating (< 5000 ft) operating (> 5000 ft) non-operating | 41° to 95° F (5° to 35° C) 41° to 86° F (5° to 30° C) -4° to 140° F (-20\xβ0 to 60° C)
Thermal Gradient: | maximum | 18° F (10° C) per hour
Altitude: | operating non-operating | 10,000 ft (3,048 m) MSL, maximum 40,000 ft (12,192 m) MSL, maximum

Table A-2. Electrical and Cooling Specifications

Parameter |  | Specification
--- | --- | ---
Voltage: |  | 187-264 Volts, 1-phase
Watts (from-the-wall): | maximum | 5750 watts
Power Factor: | minimum | 0.98
Inrush Current: | maximum | 400
Frequency: |  | 47-63 Hertz
Heat Output: | maximum | 19,550 Btu/hr (1.63 ton AC load)

Prev | Table of Contents | Next
Chapter 8. Having Trouble? |  | Index