Contents|Index|Previous|Next

# Embedded Configurations Supported

GNUPro Toolkit software supports the following embedded cross-configurations.

* Please contact your Cygnus Solutions Sales Representative for exact terms and availability on these products.

Host | Target | Output Format
SPARC Solaris 2.x | PowerPC | EABI
| M68K | a.out, COFF, VxWorks 5.1, VxWorks 5.2
| i386 | ELF
| i960 | COFF, VxWorks 5.1, VxWorks 5.2
| SH | COFF
| H8/300 | COFF
| MIPS R4 xx 0 | ELF
| MIPS R3000 | ELF, ECOFF*
| MIPS VR5000 | ELF
| SPARC | VxWorks 5.1
| SPARClet | a.out
| SPARClite | a.out, COFF
SPARC SunOS 4.1.x | PowerPC | EABI
| M68K | a.out, COFF, VxWorks 5.1, VxWorks 5.2
| i960 | COFF, VxWorks 5.1, VxWorks 5.2
| i386 | a.out, COFF, ELF
| SH | COFF
| H8/300 | COFF
| MIPS R3000 | ELF, ECOFF
| MIPS R4 xx 0 | ELF
| MIPS VR5000 | ELF
| SPARC | a.out, VxWorks 5.1
| SPARClet | a.out
| SPARClite | a.out, COFF

Host | Target | Output Format
RS6000 AIX 3.2.5 | PowerPC | EABI
| M68K | a.out
RS6000 AIX 4.1.x | PowerPC | EABI
| M68K | a.out
| i960 | VxWorks 5.1
PowerPC AIX 4.1.x | PowerPC | EABI
HP-UX 9.x/10.x | PowerPC | EABI
| M68K | a.out, COFF, VxWorks 5.1, VxWorks 5.2
| i960 | VxWorks 5.1, VxWorks 5.2
| H8/300 | COFF
| MIPS VR5000 | ELF
x86 DOS | PowerPC | EABI
| M68K | a.out, COFF
| i386 | COFF
| MIPS R3000 | ELF, ECOFF
| MIPS R4xx0 | ELF
| MIPS VR4100 | ELF
| MIPS VR4300 | ELF
| SPARC* | a.out
| SPARClite | a.out, COFF
SGI Irix 5.3 | PowerPC | EABI
| SH | COFF
| MIPS R3000 | ELF, ECOFF
| MIPS R4 xx 0 | ELF