               Hauppauge Computer Works 4860 Rescue Program
                               Version 1.0




4860RESC.COM   Saves a mirror image of the systems 128 bytes of conventional
               CMOS RAM and 8K of extended eisa CMOS RAM to files named 
               4860RESC.DAT and CONRESCU.DAT on the default drive.  This 
               program can be used to recover your CMOS RAM from diskette 
               in the event that your Hauppauge system loses battery backup. 
 
               If your Hauppauge system loses its battery backup do the 
               following:

               1) Power up system. 
               2) After the system reports configuration errors,
                  put a dos bootable diskette in drive A: and press  
                  F1 to continue.
               3) After the system boots from the diskette, insert the eisa
                  configuration disk and change to the rescue directory. 
               4) At the dos prompt type and enter 4860resc ie.
                        A:> 4860resc 
               5) After the program starts enter an " R " to restore Cmos.          

               If you have changed your systems configuration you should run  
               4860resc and save it to a diskette.  
               
               STORE THIS DISKETTE IN A SAFE PLACE.....



