    Installation of the Hauppauge TRUECOLOR Framebuffer Windows-Driver.



1.  Copy the files  FBUFFER.DRV  and  SETUP.INF 
     to your  WINDOWS\SYSTEM directory.

2.  Copy the files  WIN860.DRV  and  RUN.BAT
     to your  WINDOWS directory.

3.  In the [386enh] section of the file SYSTEM.INI
    add the following:
    EMMExclude=E000-EFFF

4.  Be sure that   APX860 V1.7  is already installed.

5.  Start  SETUP.EXE from your  WINDOWS directory.
     Choose the Hauppauge Framebuffer as display.
         
6.  Start RUN.BAT.

7.  Have lots of fun with this 16.7 MIO. COLORS.....

