[data]
type=network
version="3.11.136"

[disks]
1 = \WFW,"Port Replicator Network Drivers disk",BOXDRVR
2 = \NDIS2,"Port Replicator Network Drivers disk",BOXDRVR
3 = \ODI,"Port Replicator Network Drivers disk",BOXDRVR

[netcard]
BOXMAC=" Digital Integrated Ethernet Controller NDIS 2.01", 0, NDIS, Ethernet, REAL, BOXMAC_INST, BOXMAC_INI
BOXNDIS=" Digital Integrated Ethernet Controller NDIS 3.0", 0, NDIS, Ethernet, 0x02, BOXNDIS3_INS,BOXNDIS3_INI
BOXODI=" Digital Integrated Ethernet Controller ODI", 0, NDIS, Ethernet, 0x04, BOXODI_INST, BOXODI_INI

[BOXODI_INST]
mlid=3:boxodi.com

[BOXODI_INI]
DriverName=BOXODI$

[BOXMAC_INST]
ndis2 = 2:boxndis.dos

[BOXMAC_INI]
DriverName=BOXNDIS$
param=PS2BIDIR,"PS2BIDIRECTIONAL",keyonly,,,0x12
param=DISABLELINK,"DISABLELINK",keyonly,,,0x12
param=RJ45,"RJ45",keyonly,,,0x12
param=COAX,"COAX",keyonly,,,0x12
param=IRQ,"IRQ",enum,"3,3,4,4,5,5,7,7,10,10,11,11,12,12",11,0x10

[BOXNDIS3_INS]
ndis3 = 1:boxndis3.386

[BOXNDIS3_INI]
DriverName=BOXNDIS$
param=Port_Type,"PORT MODE",enum,"PS/2 BIDIRECTIONAL,0,EPP,1",1,0x22
param=Cable_Type,"CABLE TYPE",enum,"AUTO,0,RJ45,2,COAX,1",0,0x22
param=Disable_Link,"DISABLE LINK",enum,"YES,0,NO,16",16,0x22
param=IRQ,"IRQ",enum,"3,3,4,4,5,5,7,7,10,10,11,11,12,12",11,0x20
