; NETBOX.INF
;
; Digital HINote VP Series Network Interface Cards.
;

[version]
LayoutFile=layout.inf
signature="$CHICAGO$"
Class=Net
provider=%V_MS%

[Manufacturer]
%V_BOXER%=Boxer

[Boxer]
%*BOXSL00.DeviceDesc%=*BOXSL00.ndi, *DEC80F0 ;Digital HINote Port Replicator


;****************************************************************************
;    *BOXSL00   Boxer Port Replicator
;****************************************************************************

[*BOXSL00.ndi]
AddReg=*BOXSL00.ndi.reg,box3.ndi.reg
CopyFiles=box3.ndis3.CopyFiles

[*BOXSL00.ndi.reg]
HKR,Ndi,DeviceID,,"*DEC80F0"
;Parallel port Type Parameter
HKR,Ndi\params\Port_Type,ParamDesc,,"%BOXSL00_PARAM_PORTTYPE%
HKR,NDI\params\Port_Type,flag,1,20,00,00,00
HKR,Ndi\params\Port_Type,optional,,0
HKR,Ndi\params\Port_Type,default,,1
HKR,Ndi\params\Port_Type,type,,enum
HKR,Ndi\params\Port_Type\enum,1,,%PARAM_EPP%
HKR,Ndi\params\Port_Type\enum,0,,%PARAM_PS2BIDIR%
;Cable Type Parameter
HKR,Ndi\params\Cable_Type,ParamDesc,,"%BOXSL00_PARAM_CABLETYPE%
HKR,NDI\params\Cable_Type,flag,1,20,00,00,00
HKR,Ndi\params\Cable_Type,optional,,0
HKR,Ndi\params\Cable_Type,default,,0
HKR,Ndi\params\Cable_Type,type,,enum
HKR,Ndi\params\Cable_Type\enum,0,,%PARAM_AUTO%
HKR,Ndi\params\Cable_Type\enum,2,,%PARAM_RJ45%
HKR,Ndi\params\Cable_Type\enum,1,,%PARAM_COAX%
;Disable link Parameter
HKR,Ndi\params\Disable_Link,ParamDesc,,"%BOXSL00_PARAM_DISABLELINK%
HKR,NDI\params\Disable_Link,flag,1,20,00,00,00
HKR,Ndi\params\Disable_Link,optional,,0
HKR,Ndi\params\Disable_Link,default,,16
HKR,Ndi\params\Disable_Link,type,,enum
HKR,Ndi\params\Disable_Link\enum,0,,%PARAM_YES%
HKR,Ndi\params\Disable_Link\enum,16,,%PARAM_NO%
;IRQ number Parameter
HKR,Ndi\params\IRQ,ParamDesc,,"%BOXSL00_PARAM_IRQ%
HKR,NDI\params\IRQ,flag,1,20,00,00,00
HKR,Ndi\params\IRQ,optional,,0
HKR,Ndi\params\IRQ,default,,11
HKR,Ndi\params\IRQ,type,,enum
HKR,Ndi\params\IRQ\enum,3,,%PARAM_3%
HKR,Ndi\params\IRQ\enum,4,,%PARAM_4%
HKR,Ndi\params\IRQ\enum,5,,%PARAM_5%
HKR,Ndi\params\IRQ\enum,7,,%PARAM_7%
HKR,Ndi\params\IRQ\enum,10,,%PARAM_10%
HKR,Ndi\params\IRQ\enum,11,,%PARAM_11%
HKR,Ndi\params\IRQ\enum,12,,%PARAM_12%
HKR,Ndi\params\IRQ\enum,15,,%PARAM_15%



;****************************************************************************
;    *BOXSL00   Boxer Port Replicator
;****************************************************************************
; Base section
[box3.ndi.reg]
; key,subkey,valuname,type,value
HKR,,Ver,,2.02.00.2524
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,decndis3.vxd
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
; NDIS Info
HKR,NDIS,LogDriverName,,"BOXNDIS3"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A
; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
; Install sections
HKR,Ndi\Install,ndis3,,"box3.ndis3"

; Install NDIS3
[box3.ndis3]
CopyFiles=box3.ndis3.CopyFiles

[box3.ndis3.CopyFiles]
decndis3.vxd

;****************************************************************************
; Destination Directories
;****************************************************************************
[DestinationDirs]
DefaultDestDir              =11 ; LDID_SYS
box3.ndis3.CopyFiles        =11

[SourceDisksNames]
50="Port Replicator Network Drivers Disk","",0

[SourceDisksFiles]
decndis3.vxd=50,,

;****************************************************************************
; Localizable Strings
;****************************************************************************
[strings]
; Provider
V_MS="Microsoft"
; Manufacturers
V_Boxer="Digital Equipment"
; PNP Devices
*BOXSL00.DeviceDesc="Digital HiNote VP Series Port Replicator"


; Parameters
PARAM_PS2BIDIR="PS/2 BIDIRECTIONAL"
PARAM_EPP="EPP"
BOXSL00_PARAM_PORTTYPE="PORT MODE"
PARAM_AUTO="AUTO"
PARAM_RJ45="RJ45"
PARAM_COAX="COAX"
BOXSL00_PARAM_CABLETYPE="CABLE TYPE"
PARAM_YES="YES"
PARAM_NO="NO"
BOXSL00_PARAM_DISABLELINK="DISABLE LINK"
BOXSL00_PARAM_IRQ="IRQ"
PARAM_3="3"
PARAM_4="4"
PARAM_5="5"
PARAM_7="7"
PARAM_10="10"
PARAM_11="11"
PARAM_12="12"
PARAM_15="15"
