                    Installing Windows 95
                        Video Drivers
                              
                              
                              
                              

Requirements

HP OmniBook 800 with retail Windows 95 installed.
HP OmniBook 800 Recovery CD and CDROM drive.

Procedures

1.   Connect the OmniBook 800 CDROM drive.
2.   Insert the OmniBook Recovery CD in the CDROM drive.
3.   Run Windows 95.
4.   Open the Control Panel and double-click on Display.
5.   Go to the Setting Tab.
6.   Select Change Display Type.
7.   Under Adapter Type, select Change.
8.   Click Have Disk
9.   Go to \OMNIBOOK\DRIVERS\WIN95\VIDEO on the Recovery CD.
10.  Select nmx.inf
11.  Click OK until the Select Device window appears.
12.  Select NeoMagic NMX and click OK.
13.  Change the Monitor Type to Laptop Display Panel (800x600), click Close.
14.  Click Close in Display Properties.
15.  Click Yes to restart the System.

