                  PC Card (PCMCIA) Support



Requirements
  
HP OmniBook 800 with retail Windows 95A installed.
HP OmniBook Support Utility Disk and floppy disk drive.
HP OmniBook Recovery CD and CD-ROM drive.

NOTE:  This procedure is only to be performed on the A version of Windows
       95.  To verify what version you have, double click on the System icon
       in the Control Panel.  Under the 'General' tab you will find a System:
       field and the following information:
		
		Microsoft Windows 95
		4.00.950a

       If you see something other than that, do not perform this procedure.


Procedure

1.   Connect the OmniBook floppy disk drive and CD-ROM drive.
2.   Insert the OmniBook Support Utility Disk in the floppy disk drive.
3.   Insert the OmniBook Recovery CD in the CD-ROM drive.
4.   Reboot the OmniBook.
5.   Select MS-DOS prompt With Built in SCSI CD-ROM Support.
6.   At the DOS prompt, type G: to change to the CD-ROM drive.
7.   Type: CD \OMNIBOOK\DRIVERS\WIN95\PCCARD\95OAONLY
8.   Type: COPY *.VXD C:\WINDOWS\SYSTEM
9.   Type: COPY PCMCIA.INF C:\WINDOWS\INF
10.  Type: COPY PCMCIA.REG C:\
11.  Remove the OmniBook Support Utility Disk from the floppy disk drive
12.  Reboot the OmniBook into Windows 95.
13.  Open a DOS window
14.  Type: REGEDIT C:\PCMCIA.REG
15.  Type: DEL C:\PCMCIA.REG
16.  Reboot the OmniBook into Windows 95.

