Installing SCSI in Windows NT 3.51

System Installation Requirements:
      HP OmniBook 800 with Windows NT 3.51 installed.
      HP OmniBook 800 Microsoft Windows NT SCSI driver.  This
      driver can be found on the HP default build in the following
      directory:  C:\OMNIBOOK\DRIVERS\NT\SCSI.  This driver can
      also be found on the HP OmniBook 800 recovery CD-ROM.
     
Procedure:

1.   Boot Windows NT and log on as adminstrator.

2.   Open the Main window in Program Manager.

3.   Double-click on Windows NT Setup.

4.   Choose Options then Add/Remove SCSI Adapters.

5.   Choose to Remove the current SCSI Adapter by
  highlighting it and then choosing the Remove button.

6.   Now choose Add to add an adapter.  Scroll down to
  Other requires disk from manufacturer.  Windows NT will
  ask for the location of the driver.  Enter the path where
  the driver disks can be found.   Windows NT will find the
  Symbios Logic PCI (53c8XX) choose OK to load this
  driver.

7.   Once Windows NT has loaded the driver, you will be
  asked to reboot.  Once rebooted, the SCSI adapter will
  function correctly.


