!!!   Original (non modified) SAME version bios MUST be flashed at first !!!
_______________________________________________

Check the BIOS ID before the mod flashing !!!!

for TP-6D use TP-6D folder
for TP-7X use TP-7X folder
__________________________

for WListed mod flashing :

run the WinPhlash (as Administrator), click "Advanced Settings" then check and
uncheck the boxes so it looks like this:

("Flags" Tab):
[ ] Verify BIOS part number
[ ] Flash only if BIOS version is different
[ ] Flash only if BIOS version is newer
[ ] Verify BIOS image size
[ ] Verify BIOS checksum
[ ] Zero block before erasing
[x] Verify block after programming
[x] Disable Axx swaping automatic detection (if present)
[ ] Clear CMOS Checksum

("DMI" tab)
"Update": Select "Update the BIOS and not DMI" 
