Neko Project II
                                   Yui/Punyu/Studio Milmake 1999-2000


What is NP2
-----------

  NP2 is a NEC PC-9801 series emulator.
  Many programs don't work correctly.....


System Reuirements
------------------

  Absolute minimum system:

    - Microsoft-Windows4.00 + DirectX2 or Microsoft-Windows NT5


  Recommended System:

    - Microsoft-Windows4.00 + DirectX2 or Microsoft-Windows NT5
    - Celeron processor
    - 64MB ro RAM


Installing NP2
--------------

  1. Unzip the pack

  2. Copy FONT.BMP to the NP2 dir.
      NP2 can use the BMP file of ANEX86 and T98.
      (It may rename file by the case...)


Work NP2
--------

  - V30 (only 186 opcode)
  - 80286 (only realmode)
  - 640KB user's RAM and 1024KB Extend RAM
  - BIOS INT 08h, 09h, 13h, 18h, 1bh, 1ch
  - LIO
  - 2 floppy disk drives
         supported image: *.D88 / plane image
  - SASI hard disk
         supported image: *.THD(T98), *.HDI(ANEX86)
  - Mouse
  - PC-9801-14 (Music generator board)
  - PC-9801-26K (OPN sound board)
  - PC-9801-86 (OPNA+86PCM sound board)
  - PC-9801-118 (YMF-288+CS4231 sound board)
  - MPU-98II (MIDI board)
  - N88-BASIC (require BIOS.ROM file)


Lacks of NP2
------------

  - i286 Protect mode
  - SCSI


Extra keys
----------

  F11: System Menu
  F12: Mouse capture


